nvic: IRQControllers.NVIC @ sysbus 0xE000E000
    priorityMask: 0xF0
    systickFrequency: 32000000
    IRQ -> cpu@0

cpu: CPU.CortexM @ sysbus
    cpuType: "cortex-m33"
    nvic: nvic

// Missing interrupt lines for SPIs
spi1: SPI.STM32SPI @ sysbus 0x40013000

spi2: SPI.STM32SPI @ sysbus 0x40003800

spi3: SPI.STM32SPI @ sysbus 0x40003C00

// This model's registers are not compatible with the EXTI in this MCU,
// it is currently here to support direct interrupts
exti: IRQControllers.STM32F4_EXTI @ sysbus 0x4002F400
    [0-15,17] -> nvic@[11-26,2]
    numberOfOutputLines: 43
    firstDirectLine: 17

sram1: Memory.MappedMemory @ sysbus 0x20000000
    size: 0x30000

flash: Memory.MappedMemory @ sysbus 0x08000000
    size: 0x80000

// frequency to be verified
usart1: UART.STM32F7_USART @ sysbus 0x40013800
    frequency: 200000000
    IRQ -> nvic@61

usart2: UART.STM32F7_USART @ sysbus 0x40004400
    frequency: 200000000
    IRQ -> nvic@62

usart3: UART.STM32F7_USART @ sysbus 0x40004800
    frequency: 200000000
    IRQ -> nvic@63

uart4: UART.STM32F7_USART @ sysbus 0x40004C00
    frequency: 200000000
    IRQ -> nvic@64

uart5: UART.STM32F7_USART @ sysbus 0x40005000
    frequency: 200000000
    IRQ -> nvic@65

lpuart1: UART.STM32F7_USART @ sysbus 0x40008000
    frequency: 200000000
    IRQ -> nvic@66

gpioPortA: GPIOPort.STM32_GPIOPort @ sysbus <0x42020000, +0x400>
    modeResetValue: 0xABFFFFFF
    outputSpeedResetValue: 0x0C000000
    pullUpPullDownResetValue: 0x64000000
    numberOfAFs: 16
    invertedAFPins: [[5, 3], [7, 1, 3]]

gpioPortB: GPIOPort.STM32_GPIOPort @ sysbus <0x42020400, +0x400>
    modeResetValue: 0xFFFFFEBF
    pullUpPullDownResetValue: 0x00000100
    numberOfAFs: 16
    invertedAFPins: [[0, 1, 3], [1, 1, 3], [13, 1], [14, 1, 3], [15, 1, 3]]

gpioPortC: GPIOPort.STM32_GPIOPort @ sysbus <0x42020800, +0x400>
    modeResetValue: 0xFFFFFFFF
    numberOfAFs: 16

gpioPortD: GPIOPort.STM32_GPIOPort @ sysbus <0x42020C00, +0x400>
    modeResetValue: 0xFFFFFFFF
    numberOfAFs: 16

gpioPortE: GPIOPort.STM32_GPIOPort @ sysbus <0x42021000, +0x400>
    modeResetValue: 0xFFFFFFFF
    numberOfAFs: 16
    invertedAFPins: [[8, 1], [10, 1], [12, 1]]

gpioPortF: GPIOPort.STM32_GPIOPort @ sysbus <0x42021400, +0x400>
    modeResetValue: 0xFFFFFFFF
    numberOfAFs: 16

gpioPortG: GPIOPort.STM32_GPIOPort @ sysbus <0x42021800, +0x400>
    modeResetValue: 0xFFFFFFFF
    numberOfAFs: 16

gpioPortH: GPIOPort.STM32_GPIOPort @ sysbus <0x42021C00, +0x400>
    modeResetValue: 0x0000000F
    numberOfAFs: 16

dma1: DMA.STM32LDMA @ sysbus 0x40020000
    [0-7] -> nvic@[29-36]

i2c1: I2C.STM32F4_I2C @ sysbus 0x40005400
    EventInterrupt -> nvic@55
    ErrorInterrupt -> nvic@56

rtc: STM32L_RTC @ sysbus <0x40002800, +0x400>
    -> exti@17

timer1: Timers.STM32_Timer @ sysbus 0x40012c00
    -> nvic@42
    frequency: 10000000
    initialLimit: 0xFFFF

// frequency to be verified
timer2: Timers.STM32_Timer @ sysbus 0x40000000
    -> nvic@45
    frequency: 10000000
    initialLimit: 0xFFFFFFFF

timer3: Timers.STM32_Timer @ sysbus 0x40000400
    -> nvic@46
    frequency: 10000000
    initialLimit: 0xFFFF

timer4: Timers.STM32_Timer @ sysbus 0x40000800
    -> nvic@47
    frequency: 10000000
    initialLimit: 0xFFFF

timer5: Timers.STM32_Timer @ sysbus 0x40000C00
    -> nvic@48
    frequency: 10000000
    initialLimit: 0xFFFFFFFF

timer6: Timers.STM32_Timer @ sysbus 0x40001000
    -> nvic@49
    frequency: 10000000
    initialLimit: 0xFFFF

timer7: Timers.STM32_Timer @ sysbus 0x40001400
    -> nvic@50
    frequency: 10000000
    initialLimit: 0xFFFF

timer8: Timers.STM32_Timer @ sysbus 0x40013400
    -> nvic@52
    frequency: 10000000
    initialLimit: 0xFFFF

timer15: Timers.STM32_Timer @ sysbus 0x40014000
    -> nvic@69
    frequency: 10000000
    initialLimit: 0xFFFF

timer16: Timers.STM32_Timer @ sysbus 0x40014400
    -> nvic@70
    frequency: 10000000
    initialLimit: 0xFFFF

timer17: Timers.STM32_Timer @ sysbus 0x40014800
    -> nvic@71
    frequency: 10000000
    initialLimit: 0xFFFF

// Alternate function mapping connections. For more details see `stm32l071.repl`.
timer1:
    0 -> gpioPortA#07@01 | gpioPortA#08@01 | gpioPortB#13@01 | gpioPortE#08@01 | gpioPortE#09@01
    1 -> gpioPortA#09@01 | gpioPortB#00@01 | gpioPortB#14@01 | gpioPortE#10@01 | gpioPortE#11@01
    2 -> gpioPortA#10@01 | gpioPortB#01@01 | gpioPortB#15@01 | gpioPortE#12@01 | gpioPortE#13@01
    3 -> gpioPortA#11@01 | gpioPortE#14@01

timer2:
    0 -> gpioPortA#00@01 | gpioPortA#05@01 | gpioPortA#15@01
    1 -> gpioPortA#01@01 | gpioPortB#03@01
    2 -> gpioPortA#02@01 | gpioPortB#10@01
    3 -> gpioPortA#03@01 | gpioPortB#11@01

timer3:
    0 -> gpioPortA#06@02 | gpioPortB#04@02 | gpioPortC#06@02 | gpioPortE#03@02
    1 -> gpioPortA#07@02 | gpioPortB#05@02 | gpioPortC#07@02 | gpioPortE#04@02
    2 -> gpioPortB#00@02 | gpioPortC#08@02 | gpioPortE#05@02
    3 -> gpioPortB#01@02 | gpioPortC#09@02 | gpioPortE#06@02

timer4:
    0 -> gpioPortB#06@02 | gpioPortB#12@02
    1 -> gpioPortB#07@02 | gpioPortB#13@02
    2 -> gpioPortB#08@02 | gpioPortB#14@02
    3 -> gpioPortB#09@02 | gpioPortB#15@02

timer5:
    0 -> gpioPortB#00@02 | gpioPortF#06@02
    1 -> gpioPortB#01@02 | gpioPortF#07@02
    2 -> gpioPortB#02@02 | gpioPortF#08@02
    3 -> gpioPortB#03@02 | gpioPortF#09@02

sysbus:
    init:
        // Hard set all oscillator RDY bits
        Tag <0x40021000 4> "RCC_CR" 0x2A020402
        
        // Hard set HSI16 oscillator as system clock
        Tag <0x40021008 4> "RCC_CFGR" 0x4

        Tag <0x40007000 0x400> "PWR"
        Tag <0xE0001000 0xffb> "DWT"
