using sysbus
$name?="Microwatt"

mach create $name
machine LoadPlatformDescription @platforms/cpus/microwatt.repl

$bin?=@https://dl.antmicro.com/projects/renode/microwatt--micropython.elf-s_2282296-072a8aac5d4d9897425f72ec2ca8ca123e6d624f

showAnalyzer uart

macro reset
"""
    sysbus LoadELF $bin

    # Microwatt should always boot from 0 but the ELF files tend to set the
    # entry point differently. Adjust this to match your use case.
    cpu PC 0
"""

runMacro $reset
