using "./efr32mg12.repl"

rtcc:
    -> nvic@31

i2c1:
    -> nvic@40

usart0:
    ReceiveIRQ -> nvic@12
    TransmitIRQ -> nvic@13
usart1:
    ReceiveIRQ -> nvic@20
    TransmitIRQ -> nvic@21
usart2:
    ReceiveIRQ -> nvic@38
    TransmitIRQ -> nvic@39
usart3: @ none

sram:
    size: 0x00040000

flash:
    size: 0x00100000

wtimer0:
    frequency: 0x1000000 //bogus
    width: TimerWidth.Bit32
    -> nvic@37

wtimer1: @ none

deviceInformation:
    deviceFamily: DeviceFamily.EFR32MG13P
