using "platforms/cpus/miv.repl"

gpioOutputs:
    0 -> led0@0
    1 -> led1@0

led0: Miscellaneous.LED @ gpioOutputs 0
    invert: true

led1: Miscellaneous.LED @ gpioOutputs 1
    invert: true

user_switch_0: Miscellaneous.Button @ gpioInputs 0
    invert: true
    -> gpioInputs@0

user_switch_1: Miscellaneous.Button @ gpioInputs 1
    invert: true
    -> gpioInputs@1

user_switch_2: Miscellaneous.Button @ gpioInputs 2
    invert: true
    -> gpioInputs@2
