using "platforms/cpus/eos-s3.repl"

intrCtrl:
    3 -> ledB@0
    1 -> ledG@0
    0 -> ledR@0

ledB: Miscellaneous.LED @ intrCtrl 3

ledG: Miscellaneous.LED @ intrCtrl 1

ledR: Miscellaneous.LED @ intrCtrl 0

uart: @ none

usbserial: UART.USBSerialPort_S3B @ { sysbus 0x40020000 }
