using sysbus

# create the platform
mach create
machine LoadPlatformDescription @platforms/cpus/xtensa-sample-controller.repl

# display the UART analyzer window
showAnalyzer cpu.uartSemihosting

# load the ELF file
macro reset
"""
    sysbus LoadELF @https://dl.antmicro.com/projects/renode/xtensa-sample-controller-zephyr-hello-world.elf-s_293544-4be60f8a3891e70c30e1e8a471df4ad12ab08144
"""
runMacro $reset

