using "platforms/cpus/eos-s3.repl"

intrCtrl:
    4 -> ledB@0
    5 -> ledG@0
    6 -> ledR@0

user_button: Miscellaneous.Button @ intrCtrl 1
    invert: true
    -> intrCtrl@31

ledB: Miscellaneous.LED @ intrCtrl 4

ledG: Miscellaneous.LED @ intrCtrl 5

ledR: Miscellaneous.LED @ intrCtrl 6

mc3635: Sensors.MC3635 @ i2cMaster0 0x4c
