:name: cc2538 range medium 3 nodes

######################################################################
#
# Sample script creating 1 server node and 2 client nodes using a
# range-based medium function - transmission is possible if nodes are
# in range. Nodes are positioned in a 3D space (x,y,z),
# at a distance of 10 (units) from each other.
#
######################################################################

emulation CreateIEEE802_15_4Medium "wireless"

# The radio is using a range-based medium (with the `Range` set to `11`)
# If not set, the default SimpleMediumFunction will be used (where range is not relevant)
wireless SetRangeWirelessFunction 11

######################### UDP SERVER - begin #########################
$bin=@https://dl.antmicro.com/projects/renode/udp-server.elf-s_173732-a2aefb896d521a8fdc2a052cac1933c68cc39bf5
$name="server"
i @scripts/single-node/cc2538.resc
connector Connect radio wireless
wireless SetPosition radio 0 0 0
mach clear
########################## UDP SERVER - end ##########################

######################### UDP CLIENT - begin #########################
$bin=@https://dl.antmicro.com/projects/renode/udp-client.elf-s_173840-9eed7fe31993d055b98410b886044e8205a95644
$name="client-1"
i @scripts/single-node/cc2538.resc
connector Connect radio wireless
wireless SetPosition radio 10 0 0
mach clear
########################## UDP CLIENT - end ##########################

######################### UDP CLIENT - begin #########################
$name="client-2"
i @scripts/single-node/cc2538.resc
connector Connect radio wireless
wireless SetPosition radio 0 10 0
mach clear
########################## UDP CLIENT - end ##########################
