:name: Zynqmp
:description: This script runs Linux on Zynq UltraScale+ MPSoC.

using sysbus
using sysbus.cluster0
using sysbus.cluster1

$name?="ZynqUS+"
mach create $name

machine LoadPlatformDescription @platforms/cpus/zynqmp.repl
showAnalyzer uart1

$dtb?=       @https://dl.antmicro.com/projects/renode/zynq-us_plus--sm-k26-revA.dtb-s_37854-cc08802e65ac86f1415bfd58b5bfc2f2fbc9c3f0
$atf_elf?=   @https://dl.antmicro.com/projects/renode/zynq-us_plus--bl31.elf-s_770984-aad9c28d989600caa8fd436bca66eb500e0606dd
$uboot?=     @https://dl.antmicro.com/projects/renode/zynq-us_plus--u-boot.bin-s_1351888-8291c2fd5e7fed3bda101e4c0694991fb40af277
$uboot_elf?= @https://dl.antmicro.com/projects/renode/zynq-us_plus--u-boot.elf-s_1418000-23d4b0115d096ce9ed85c7e146f687a528382326
$linux?=     @https://dl.antmicro.com/projects/renode/zynq-us_plus--linux.Image-s_21039616-74b4831df919e21f699cc0d647874bfa99d69fb6
$linux_elf?= @https://dl.antmicro.com/projects/renode/zynq-us_plus--vmlinux-s_26614776-efb126bb528fb25d022b3cec1c1a08d555608e65
$rootfs?=    @https://dl.antmicro.com/projects/renode/zynq-us_plus--rootfs.ext2-s_62914560-3d4dd1f233b7be349e7ec48d64d6081cb5350d77

macro reset
"""
    # Only set PC for and start the primary core - secondaries are handled by firmware during wakeup
    apu0 PC 0x1000000
    cluster0 ForEach IsHalted true
    apu0 IsHalted false

    cluster1 ForEach IsHalted true

    sysbus LoadELF    $atf_elf cpu=apu0

    sysbus LoadFdt    $dtb    0x100000   "earlycon console=ttyPS1,115200n8 root=/dev/ram0 rw initrd=0x20000000,64M" false
    sysbus LoadBinary $uboot  0x8000000
    sysbus LoadBinary $linux  0x10000000
    sysbus LoadBinary $rootfs 0x20000000

    sysbus LoadSymbolsFrom $uboot_elf
    sysbus LoadSymbolsFrom $linux_elf
"""

runMacro $reset
