:name: Zynqmp
:description: This script runs on Zynq UltraScale+ MPSoC. It's showcasing two way communication between Linux running on Cortex-A53 and OpenAMP demo running on Cortex-R5.

using sysbus
using sysbus.cluster0
using sysbus.cluster1

$name?="ZynqUS+"
mach create $name

machine LoadPlatformDescription @platforms/cpus/zynqmp.repl
machine SetSerialExecution True
showAnalyzer uart1

$dtb?=       @https://dl.antmicro.com/projects/renode/zynqmp--sm-k26-revA-openamp.dtb-s_39685-7bc435ab006028eab6e7da35bff8f7ce891cfce9
$atf_elf?=   @https://dl.antmicro.com/projects/renode/zynq-us_plus--bl31.elf-s_770984-aad9c28d989600caa8fd436bca66eb500e0606dd
$uboot?=     @https://dl.antmicro.com/projects/renode/zynq-us_plus--u-boot.bin-s_1351888-8291c2fd5e7fed3bda101e4c0694991fb40af277
$uboot_elf?= @https://dl.antmicro.com/projects/renode/zynq-us_plus--u-boot.elf-s_1418000-23d4b0115d096ce9ed85c7e146f687a528382326
$linux?=     @https://dl.antmicro.com/projects/renode/zynqmp--linux-Image-openamp-s_23429632-e9ff8dd5c5963153dd87791cc250dea3c039cbbc
$linux_elf?= @https://dl.antmicro.com/projects/renode/zynq-us_plus--vmlinux-s_26614776-efb126bb528fb25d022b3cec1c1a08d555608e65
$rootfs?=    @https://dl.antmicro.com/projects/renode/zynqmp--linux-rootfs-openamp.ext2-s_62914560-56183cdaeef8af742ea31ee9044b733ccf49c0d1

macro reset
"""
    apu0 PC 0x1000000
    cluster0 ForEach IsHalted true
    apu0 IsHalted false

    cluster1 ForEach IsHalted true

    sysbus LoadELF    $atf_elf cpu=apu0

    sysbus LoadFdt    $dtb    0x100000   "earlycon console=ttyPS1,115200n8 root=/dev/ram0 rw initrd=0x20000000,64M" false context=apu0
    sysbus LoadBinary $uboot  0x8000000  cpu=apu0
    sysbus LoadBinary $linux  0x10000000 cpu=apu0
    sysbus LoadBinary $rootfs 0x20000000 cpu=apu0

    sysbus LoadSymbolsFrom $uboot_elf context=apu0
    sysbus LoadSymbolsFrom $linux_elf context=apu0
"""

runMacro $reset
