// Main Flash memory
// Upper size:
// STM32G0B1xx and STM32G0C1xx: 0x0807 FFFF; STM32G071xx and STM32G081xx: 0x0801 FFFF; STM32G051xx and
// STM32G061xx, STM32G031xx and STM32G041xx: 0x0800 FFFF.
flash: Memory.MappedMemory @ sysbus 0x08000000
    size: 0x20000

ram: Memory.MappedMemory @ sysbus 0x20000000
    size: 0xC000

nvic: IRQControllers.NVIC @ sysbus 0xE000E000
    priorityMask: 0xF0
    systickFrequency: 72000000
    IRQ -> cpu@0

// This model's registers are not compatible with the EXTI in this MCU,
// it is currently here to support direct interrupts
exti: IRQControllers.STM32F4_EXTI @ sysbus 0x40021800
    numberOfOutputLines: 34
    firstDirectLine: 19
    [0, 1] -> nvicInput5@[0, 1]
    [2, 3] -> nvicInput6@[0, 1]
    [4-15] -> nvicInput7@[0-11]
    [23] -> nvic@[23]
    [32, 33] -> nvicInput8@[0, 1]
    [17, 18] -> nvicInput12@[0, 1]

nvicInput8: Miscellaneous.CombinedInput @ none
    numberOfInputs: 2
    -> nvic@8

nvicInput10: Miscellaneous.CombinedInput @ none
    numberOfInputs: 2
    -> nvic@10

nvicInput11: Miscellaneous.CombinedInput @ none
    numberOfInputs: 9
    -> nvic@11

nvicInput12: Miscellaneous.CombinedInput @ none
    numberOfInputs: 2
    -> nvic@12

nvicInput5: Miscellaneous.CombinedInput @ none
    numberOfInputs: 2
    -> nvic@5

nvicInput6: Miscellaneous.CombinedInput @ none
    numberOfInputs: 2
    -> nvic@6

nvicInput7: Miscellaneous.CombinedInput @ none
    numberOfInputs: 12
    -> nvic@7

nvicInput29: Miscellaneous.CombinedInput @ none
    numberOfInputs: 4
    -> nvic@29

cpu: CPU.CortexM @ sysbus
    cpuType: "cortex-m0"
    nvic: nvic

usart1: UART.STM32F7_USART @ sysbus 0x40013800
    frequency: 200000000
    IRQ -> nvic@27

usart2: UART.STM32F7_USART @ sysbus 0x40004400
    frequency: 200000000
    IRQ -> nvic@28

usart3: UART.STM32F7_USART @ sysbus 0x40004800
    frequency: 200000000
    IRQ -> nvicInput29@0

usart4: UART.STM32F7_USART @ sysbus 0x40004C00
    frequency: 200000000
    IRQ -> nvicInput29@1

usart5: UART.STM32F7_USART @ sysbus 0x40005000
    frequency: 200000000
    IRQ -> nvicInput29@2

usart6: UART.STM32F7_USART @ sysbus 0x40013C00
    frequency: 200000000
    IRQ -> nvicInput29@3

gpioPortA: GPIOPort.STM32_GPIOPort @ sysbus <0x50000000, +0x400>
    modeResetValue: 0xEBFFFFFF
    pullUpPullDownResetValue: 0x24000000
    numberOfAFs: 8
    invertedAFPins: [[7, 2]]
    [0-15] -> exti@[0-15]

gpioPortB: GPIOPort.STM32_GPIOPort @ sysbus <0x50000400, +0x400>
    modeResetValue: 0xFFFFFFFF
    pullUpPullDownResetValue: 0x00000000
    numberOfAFs: 8
    invertedAFPins: [[0, 2], [1, 2], [6, 2], [7, 2], [13, 2], [14, 2], [15, 2]]
    [0-15] -> exti@[0-15]

gpioPortC: GPIOPort.STM32_GPIOPort @ sysbus <0x50000800, +0x400>
    modeResetValue: 0xFFFFFFFF
    pullUpPullDownResetValue: 0x00000000
    numberOfAFs: 8
    [0-15] -> exti@[0-15]

gpioPortD: GPIOPort.STM32_GPIOPort @ sysbus <0x50000C00, +0x400>
    modeResetValue: 0xFFFFFFFF
    pullUpPullDownResetValue: 0x00000000
    numberOfAFs: 8
    invertedAFPins: [[2, 2], [3, 2]]
    [0-15] -> exti@[0-15]

gpioPortE: GPIOPort.STM32_GPIOPort @ sysbus <0x50001000, +0x400>
    modeResetValue:0xFFFFFFFF
    pullUpPullDownResetValue: 0x00000000
    numberOfAFs: 8
    [0-15] -> exti@[0-15]

gpioPortF: GPIOPort.STM32_GPIOPort @ sysbus <0x50001400, +0x400>
    modeResetValue: 0xFFFFFFFF
    pullUpPullDownResetValue: 0x00000000
    numberOfAFs: 8
    [0-15] -> exti@[0-15]

i2c1: I2C.STM32F7_I2C @ sysbus 0x40005400
    EventInterrupt -> exti@23

i2c2: I2C.STM32F7_I2C @ sysbus 0x40005800
    EventInterrupt -> exti@22

spi1: SPI.STM32SPI @ sysbus 0x40013000
    IRQ -> nvic@25

spi2: SPI.STM32SPI @ sysbus 0x40003800
    IRQ -> nvic@26

spi3: SPI.STM32SPI @ sysbus 0x40003C00
    IRQ -> nvic@26

timer1: Timers.STM32_Timer @ sysbus 0x40012C00
    frequency: 10000000
    initialLimit: 0xFFFF
    [BreakInterrupt, UpdateInterrupt, TriggerInterrupt, CommutationInterrupt] -> nvic@[13, 13, 13, 13]
    CaptureCompareInterrupt -> nvic@14

timer2: Timers.STM32_Timer @ sysbus 0x40000000
    frequency: 10000000
    initialLimit: 0xFFFFFFFF
    -> nvic@15

timer3: Timers.STM32_Timer @ sysbus 0x40000400
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@16

timer4: Timers.STM32_Timer @ sysbus 0x40000800
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@16

timer6: Timers.STM32_Timer @ sysbus 0x40001000
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@17

timer7: Timers.STM32_Timer @ sysbus 0x40001400
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@18

timer14: Timers.STM32_Timer @ sysbus 0x40002000
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@19

timer15: Timers.STM32_Timer @ sysbus 0x40014000
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@20

timer16: Timers.STM32_Timer @ sysbus 0x40014400
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@21

timer17: Timers.STM32_Timer @ sysbus 0x40014800
    frequency: 10000000
    initialLimit: 0xFFFF
    -> nvic@22

fdcan1: CAN.STMCAN @ sysbus <0x40006400, +0x400>
fdcan2: CAN.STMCAN @ sysbus <0x40006800, +0x400>

rtc: Timers.STM32F4_RTC @ sysbus 0x40002800
    AlarmIRQ -> exti@19

rcc: Python.PythonPeripheral @ sysbus 0x40021000
    size: 0x400
    initable: true
    script: '''
if request.IsInit:
   lastVal = 0
   data = {'hsion': 1, 'pllon': 0, 'sw': 0, 'lsion': 0}
self.NoisyLog("%s on FLIPFLOP at offset 0x%x, value 0x%x, length %d, %s" % (str(request.Type), request.Offset, request.Value, request.Length, str(data)))

if request.IsWrite:
    if request.Offset == 0x0:
        # HSION [doc = "Bit 8 - HSI16 clock enable"]
        data['hsion'] = (request.Value >> 8) & 0x1
        # PLLON [doc = "Bit 24 - PLL enable"]
        data['pllon'] = (request.Value >> 24) & 0x1
    elif request.Offset == 0x8:
        # SW_W [doc = "Bits 0:2 - System clock switch"]
        data['sw'] = request.Value & 0x7
    elif request.Offset == 0x60:
        data['lsion'] = request.Value & 0x1
elif request.IsRead:
    lastVal = 1 - lastVal
    if request.Offset == 0x0:
        # request.Value = lastVal * 0x83

        # RCC_CR [doc = "0x00 - Clock control register"]
        # HSION_RW [doc = "Bit 8 - HSI16 clock enable flag"]
        # HSIRDY_R [doc = "Bit 10 - HSI16 clock ready flag"] # HSIRDY == HISON for this model
        # PLLRDY [doc = "Bit 25 - PLL clock ready flag"]
        request.Value = (data['hsion'] << 8) | (data['hsion'] << 10) | (data['pllon'] << 25)
    elif request.Offset == 0x4:
        request.Value = lastVal * 0xFFFFFFF8
    elif request.Offset == 0x24:
        request.Value = 0x0
    elif request.Offset == 0x60:
        request.Value = (data['lsion'] << 1)
    else:
        # RCC_CFGR [doc = "0x08 - Clock configuration register"]
        # SWS_R [doc = "Bits 3:5 - System clock switch status"]
        # request.Value = lastVal * 0xFFFFFFFF
        request.Value = data['sw'] << 3

self.NoisyLog("  0x%x (%s)" % (request.Value, str(data)))
'''

dma1: DMA.STM32G0DMA @ sysbus 0x40020000
    numberOfChannels: 7
    0 -> nvic@9
    [1, 2] -> nvicInput10@[0, 1]
    [3-6] -> nvicInput11@[0-3]

dma2: DMA.STM32G0DMA @ sysbus 0x40020400
    numberOfChannels: 5
    [0-4] -> nvicInput11@[4-8]

adc: Analog.STM32G0_ADC @ sysbus 0x40012400
    referenceVoltage: 3.3
    externalEventFrequency: 1000
    -> nvic@12

iwdg: Timers.STM32_IndependentWatchdog @ sysbus 0x40003000
    frequency: 32000

flash_ctrl: MTD.STM32F4_FlashController @ sysbus 0x40022000
    flash: flash

// Alternate function mapping connections. For more details see `stm32l071.repl`.
timer1:
    0 -> gpioPortA#07@2 | gpioPortA#08@2 | gpioPortB#13@2 | gpioPortD#02@2
    1 -> gpioPortA#09@2 | gpioPortB#00@2 | gpioPortB#03@1 | gpioPortB#14@2 | gpioPortD#03@2
    2 -> gpioPortA#10@2 | gpioPortB#01@2 | gpioPortB#06@1 | gpioPortB#15@2
    3 -> gpioPortA#11@2

timer2:
    0 -> gpioPortA#00@2 | gpioPortA#05@2 | gpioPortA#15@2
    1 -> gpioPortA#01@2 | gpioPortB#03@2
    2 -> gpioPortA#02@2 | gpioPortB#10@2 | gpioPortC#06@2
    3 -> gpioPortA#03@2 | gpioPortB#11@2 | gpioPortC#07@2

timer3:
    0 -> gpioPortA#06@1 | gpioPortB#04@1 | gpioPortC#06@1
    1 -> gpioPortA#07@1 | gpioPortB#05@1 | gpioPortC#07@1
    2 -> gpioPortB#00@1
    3 -> gpioPortB#01@1

timer14:
    0 -> gpioPortA#04@4 | gpioPortA#07@4 | gpioPortB#01@0 | gpioPortF#00@2

timer16:
    0 -> gpioPortA#06@5 | gpioPortB#06@2 | gpioPortB#08@2 | gpioPortD#00@2

timer17:
    0 -> gpioPortA#07@5 | gpioPortB#07@2 | gpioPortB#09@2 | gpioPortD#01@2

sysbus:
    init:
        Tag <0x40002C00, 0x40002FFF> "WWDG"
        Tag <0x40003000, 0x400033FF> "IWDG"
        Tag <0x40005C00, 0x40005FFF> "USB "
        Tag <0x40006C00, 0x40006FFF> "CRS"
        Tag <0x40007000, 0x400073FF> "PWR"
        Tag <0x40007400, 0x400077FF> "DAC"
        Tag <0x40007800, 0x40007BFF> "CEC"
        Tag <0x40010000, 0x400103FF> "SYSCFG"
        Tag <0x40015800, 0x40015BFF> "DBG"
        Tag <0x40022000, 0x400223FF> "FLASH_INTERFACE"
        Tag <0x40023000, 0x400233FF> "CRC"
