// PowerPc needs a big-endian bus even if running in LE
sysbus:
    Endianess: Endianess.BigEndian

rom: Memory.MappedMemory @ sysbus 0x0
    size: 0x8000

sram: Memory.MappedMemory @ sysbus 0x01000000
    size: 0x00001000

main_ram: Memory.MappedMemory @ sysbus 0x40000000
    size: 0x20000000

uart: UART.LiteX_UART64 @ sysbus 0xC0001800

cpu: CPU.PowerPc64 @ sysbus
    endianness: Endianess.LittleEndian

timer0: Timers.LiteX_Timer64 @ sysbus 0xC0002000
    frequency: 100000000
    -> cpu@0

sysbus:
    init:
        Tag <0xC0000000, 0xC0000048> "CTRL"
        Tag <0xC0001000, 0xC0001800> "IDENT_MEM"
        Tag <0xc0002800, 0xC0002850> "DDR_PHY"
        Tag <0xC0003000, 0xC0003200> "SDRAM_CONTROLLER"
        Tag <0xC0001000, 0xC0001200> "UART_PHY"