using "./litex_common.repl"

cpu: CPU.PicoRV32 @ sysbus
    cpuType: "rv32imc"

timer0: Timers.LiteX_Timer @ sysbus 0xE0002000
    frequency: 100000000

uart:
    txFifoCapacity: 0 // Disable UART buffering for compatibility with older firmware
    -> cpu@3

timer0:
    -> cpu@4

eth:
    -> cpu@5

