using "./stm32f4.repl"

ltdc: Video.STM32LTDC @ sysbus 0x40016800
    -> nvic@88

memoryBank1: Memory.MappedMemory @ sysbus 0xC0000000
    size: 0x10000000

sysbus:
    init:
        ApplySVD @https://dl.antmicro.com/projects/renode/svd/STM32F429x.svd.gz
